{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Hoja1","Hoja3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Hoja1","index":0,"n_rows":15,"n_cols":11,"rows_kept":15,"cut":false,"hidden":false,"merged":[]}
["Tags","Circuito","Equipo","Descripción","Situación","Causa","SDT","Último Cambio","Comentario","Estado","Prioridad"]
["AK3-VALV-0002","Carga al D-1","AK3-FV-0002","Val.Bloqueo L.B , olefinas de unidad","L.B Sur",null,null,"27/05/2017 13:11:10",null,"Normal"]
["AK3-VALV-0003","Carga al D-1","AK3-PV-0002","Val.Bloqueo L.B , exceso olefinas  a almacenamiento","L.B Sur",null,null,"27/05/2017 13:11:21",null,"Normal"]
["AK3-VALV-0004","Carga al D-1","AK3-FV-0002","Val.Bloqueo L.B , olefinas a ET-3","L.B Norte",null,null,"27/05/2017 11:38:38",null,"Normal"]
["AK3-PT-0001","D-1","AK3-D-0001","Presión del D-1","Estructura A, suelo",null,null,"27/05/2017 11:12:40",null,"Normal"]
["AK3-PSV-0001","D-1","AK3-D-0001","PSV del D-1","Estructura A, 2ª planta",null,null,"27/05/2017 11:12:40",null,"Normal"]
["AK3-LG-0003","D-1","AK3-D-0001","Nivel del tetón del D-1","Estructura A, suelo",null,null,"27/05/2017 11:12:40",null,"Normal"]
["AK3-MOV-0009","D-1","AK3-D-0001","Val.Corte emergencia fondo D-1","Estructura A, suelo",null,null,"27/05/2017 13:11:33",null,"Normal"]
["AK3-E-0004","T-1","AK3-E-0004","Calentador de fondo de torre, vapor 50#","Estructura A, suelo",null,null,"27/05/2017 13:10:51",null,"Normal"]
["AK3-D-0102","T-1","AK3-E-0004","Deposito de condensado del E-4","Estructura A, suelo",null,201478,"27/05/2017 11:12:40",null,"Normal"]
["AK3-E-0005","Cabeza T-1","AK3-D-0002","Refrigerador de cabeza de T-1","Estructura A, suelo",null,null,"28/05/2017 11:42:31",null,"Normal"]
["AK3-D-0002","Cabeza T-1","AK3-D-0002","Deposito cabeza T-1","Estructura A, suelo",null,null,"28/05/2017 12:09:40","Bloqueado","Normal"]
["AK3-PSV-0006","Cabeza T-1","AK3-D-0002","PSV del D-2","Estructura A, suelo",null,null,"27/05/2017 11:12:40",null,"Normal"]
["AK3-FT-0012","Cabeza T-1","AK3-D-0002","Medidor incondensables a F.Gas","Estructura A, suelo",null,null,"27/05/2017 11:12:40",null,"Normal"]
["AK3-PV-0017","Cabeza T-1","AK3-D-0002","Control de presión de la T-1/D-2","Estructura A, suelo",null,null,"28/05/2017 11:50:01",null,"Normal"]

{"sheet":"Hoja3","index":1,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[]}
["Tags","Circuito","Equipo","Descripción","Situación","Causa","SDT","Último Cambio","Comentario","Estado","Prioridad"]
["AK3-VALV-0001","Carga al D-1","AK3-LV-0002","Val.Bloqueo L.B, olefinas de unidad","L.B Norte","","","2017-05-26T19:18:59",null,"Normal",1]
["AK3-VALV-0002","Carga al D-1","AK3-FV-0002","Val.Bloqueo L.B , olefinas de unidad","L.B Sur",null,null,"2017-05-27T13:11:10","","Normal",2]
["AK3-VALV-0003","Carga al D-1","AK3-PV-0002","Val.Bloqueo L.B , exceso olefinas  a almacenamiento","L.B Sur",null,null,"2017-05-27T13:11:21","","Normal",2]
["AK3-VALV-0004","Carga al D-1","AK3-FV-0002","Val.Bloqueo L.B , olefinas a ET-3","L.B Norte",null,null,"2017-05-27T11:38:38","","Normal",2]
["AK3-FT-0002","Carga al D-1","AK3-FV-0002","Alimentación de olefinas de almacenamiento","Pasillo bombas acida, sur",null,201546,"2017-05-22T19:05:00",null,"Normal",1]
["AK3-FV-0002","Carga al D-1","AK3-FV-0002","Alimentación de olefinas de almacenamiento","Pasillo bombas acida, sur",null,null,"2017-05-26T19:46:06",null,"Normal",1]
["AK3-PT-0002","Carga al D-1","AK3-PV-0002","Exceso olefinas a almacenamiento","Pasillo bombas acida, sur",null,null,"2017-05-22T19:04:54",null,"Normal",1]
["AK3-PV-0002","Carga al D-1","AK3-PV-0002","Exceso olefinas a almacenamiento","Pasillo bombas acida","",null,"2017-05-27T11:12:40","Bloqueado","Normal",3]
["AK3-FT-0003","Carga al D-1","AK3-PV-0002","Exceso olefinas a almacenamiento","Pasillo bombas acida",null,null,"2017-05-27T11:12:40",null,"Normal",3]
["AK3-LV-0002","Carga al D-1","AK3-LV-0002","Carga entrada al D-1","Estructura A, suelo","SDT",null,"2017-05-28T09:25:15","","No Normal/SDT",3]
["AK3-D-0001","D-1","AK3-D-0001","Deposito de alimentacion de carga olefinica","Estructura A, suelo","",null,"2017-05-27T11:43:46","","Normal",4]
["AK3-LT-0002","D-1","AK3-D-0001","Nivel del D-1","Estructura A, suelo","",null,"2017-05-27T11:31:15","","Normal",4]
["AK3-PT-0001","D-1","AK3-D-0001","Presión del D-1","Estructura A, suelo",null,null,"2017-05-27T11:12:40",null,"Normal",2]
["AK3-PSV-0001","D-1","AK3-D-0001","PSV del D-1","Estructura A, 2ª planta",null,null,"2017-05-27T11:12:40",null,"Normal",2]
["AK3-LG-0003","D-1","AK3-D-0001","Nivel del tetón del D-1","Estructura A, suelo",null,null,"2017-05-27T11:12:40",null,"Normal",2]
["AK3-MOV-0009","D-1","AK3-D-0001","Val.Corte emergencia fondo D-1","Estructura A, suelo","",null,"2017-05-27T13:11:33","","Normal",2]
["AK3-P-0001-A","Carga al T-1","AK3-P-0001-A","Bomba de carga a T-1","Pasillo bombas no acida","",null,"2017-05-28T12:55:12","","Normal",4]
["AK3-P-0001-B","Carga al T-1","AK3-P-0001-B","Bomba de carga a T-1","Pasillo bombas no acida","Proceso",215285,"2017-05-28T12:55:40","By-pass despegado","No Normal/Proceso",1]
["AK3-FO-0068","Carga al T-1","AK3-P-0001-A/B","Recirculación de P-1´s al D-1","Estructura A, 1ª planta",null,null,"2017-05-27T11:12:40",null,"Normal",1]
["AK3-FT-0004-A","Carga al T-1","AK3-FV-0004","Carga a la T-1","Estructura A, suelo",null,null,"2017-05-27T11:12:40","Bloqueado","Normal",1]
["AK3-E-0001","Carga al T-1","AK3-E-0001","Cambiador carga/fondo","Estructura A, suelo","",null,"2017-05-27T13:37:58","","Normal",3]
["AK3-E-0002","Carga al T-1","AK3-E-0002","Calentador de carga , vapor de 50#","Estructura A, suelo","",null,"2017-05-27T12:37:39","","Normal",3]
["AK3-D-0101","Carga al T-1","AK3-E-0002","Deposito de condensado del E-2","Estructura A, suelo",null,null,"2017-05-27T11:12:40",null,"Normal",3]
["AK3-PSV-0004","Carga al T-1","AK3-E-0002","PSV de la linea de carga a la T-1","Estructura A, suelo",null,217846,"2017-05-27T11:12:40",null,"Normal",3]
["AK3-TT-0003","Carga al T-1","AK3-E-0002","Temperatura de carga a la T-1","Estructura A, 1ª planta",null,null,"2017-05-27T11:12:40",null,"Normal",3]
["AK3-FV-0004","Carga al T-1","AK3-FV-0004","Alimentación a la T-1","Estructura A, suelo","",null,"2017-05-27T12:15:14","By-pass despegado","Normal",4]
["AK3-T-0001","T-1","AK3-T-0001","Torre de corte de olefinas","Estructura A, suelo","",null,"2017-05-27T13:00:10","","Normal",4]
["AK3-LT-0008","T-1","AK3-T-0001","Control de nivel de la T-1","Estructura A, suelo","",null,"2017-05-27T13:20:25","Bloqueado","Normal",4]
["AK3-E-0004","T-1","AK3-E-0004","Calentador de fondo de torre, vapor 50#","Estructura A, suelo","",null,"2017-05-27T13:10:51","","Normal",2]
["AK3-D-0102","T-1","AK3-E-0004","Deposito de condensado del E-4","Estructura A, suelo",null,201478,"2017-05-27T11:12:40",null,"Normal",2]
["AK3-D-0021","T-1","AK3-D-0021","Deposito de recogida de agua de la carga a T-1","Estructura A, suelo",null,null,"2017-05-27T11:12:40",null,"Normal",4]
["AK3-LT-0011","T-1","AK3-D-0021","Nivel de agua del D-21","Estructura A, suelo","",null,"2017-05-27T12:51:10","","Normal",4]
["AK3-TI-0017","T-1","AK3-T-0001","Temperatura entrada reflujo de la T-1","Estructura A, suelo",null,null,"2017-05-27T11:12:40",null,"Normal",4]
["AK3-TI-0239","Fondo T-1","AK3-T-0001","Temperatura salida fondo de la T-1","Estructura A, suelo",null,null,"2017-05-27T11:12:40",null,"Normal",3]
["AK3-MOV-0004","Fondo T-1","AK3-T-0001","Val.Corte emergencia fondo T-1","Estructura A, suelo","",null,"2017-05-27T13:30:20","","Normal",1]
["AK3-TI-0002","Fondo T-1","AK3-E-0001","Temperatura salida fondo del E-1","Estructura A, suelo",null,null,"2017-05-27T11:12:40",null,"Normal",1]
["AK3-E-0003","Fondo T-1","AK3-E-0003","Cambiador C.W fondo T-1","Estructura A, suelo","",null,"2017-05-27T13:43:52","By-pass despegado","Normal",1]
["AK3-FT-0005","Fondo T-1","AK3-FV-0005","Medidor olefinas al X-1/almacenamiento","Estructura A, suelo",null,null,"2017-05-27T11:12:40",null,"Normal",3]
["AK3-FV-0005","Fondo T-1","AK3-FV-0005","Automatica fondo T-1 al X-1/almacenamiento","Estructura A, suelo","",null,"2017-05-28T09:35:01","","Normal",3]
["AK3-PSV-0007","Cabeza T-1","AK3-T-0001","PSV de la T-1","Estructura A, suelo",null,null,"2017-05-27T11:12:40",null,"Normal",4]
["AK3-TI-0015","Cabeza T-1","AK3-T-0001","Temperatura salida cabeza de T-1","Estructura A, suelo",null,null,"2017-05-27T11:12:40",null,"Normal",4]
["AK3-PSH-0271","Cabeza T-1","AK3-T-0001","Disparo alta presión de la T-1","Estructura A, suelo",null,null,"2017-05-27T11:12:40","By-pass despegado","Normal",4]
["AK3-FV-0010","Cabeza T-1","AK3-T-0001","Control de inyección agua de calderas","Estructura A, suelo","",null,"2017-05-28T09:53:08","","Normal",1]
["AK3-E-0005","Cabeza T-1","AK3-D-0002","Refrigerador de cabeza de T-1","Estructura A, suelo","",null,"2017-05-28T11:42:31","","Normal",2]
["AK3-D-0002","Cabeza T-1","AK3-D-0002","Deposito cabeza T-1","Estructura A, suelo","",null,"2017-05-28T12:09:40","Bloqueado","Normal",2]
["AK3-PSV-0006","Cabeza T-1","AK3-D-0002","PSV del D-2","Estructura A, suelo",null,null,"2017-05-27T11:12:40",null,"Normal",2]
["AK3-PT-0017","Cabeza T-1","AK3-D-0002","Presión del D-2","Estructura A, suelo",null,null,"2017-05-27T11:12:40",null,"Normal",1]
["AK3-FT-0012","Cabeza T-1","AK3-D-0002","Medidor incondensables a F.Gas","Estructura A, suelo",null,null,"2017-05-27T11:12:40",null,"Normal",2]
["AK3-PV-0017","Cabeza T-1","AK3-D-0002","Control de presión de la T-1/D-2","Estructura A, suelo","",null,"2017-05-28T11:50:01","","Normal",2]
["AK3-LT-0013","Cabeza T-1","AK3-D-0002","Control nivel D-2","Estructura A, suelo","",null,"2017-05-28T12:00:27","","Normal",1]
["AK3-LT-0015","Cabeza T-1","AK3-D-0002","Control nivel tetón D-2","Estructura A, suelo",null,null,"2017-05-27T11:12:40","By-pass despegado","Normal",3]
["AK3-LV-0015","Cabeza T-1","AK3-D-0002","Aut. de control nivel tetón D-2 a ET-3/sumidero","Estructura A, suelo","",null,"2017-05-28T12:15:55","Bloqueado","Normal",4]
["AK3-P-0002-A","Cabeza T-1","AK3-P-0002-A","Bomba de reflujo a T-1","Estructura A, suelo","",null,"2017-05-28T13:06:12","","Normal",1]
["AK3-P-0002-B","Cabeza T-1","AK3-P-0002-B","Bomba de reflujo a T-1","Estructura A, suelo","",null,"2017-05-28T13:06:35","","No Normal/Proceso",1]
["AK3-FV-0011","Cabeza T-1","AK3-FV-0011","Aut. de control reflujo a T-1","Estructura A, suelo",null,null,"2017-05-28T12:39:56","Bloqueado","Normal",1]